

Mark Scheme (Results)

Summer 2019

Pearson Edexcel GCE

In Mathematics (8MA0) Paper 2 Mechanics

**Edexcel and BTEC Qualifications**

Edexcel and BTEC qualifications are awarded by Pearson, the UK’s largest awarding body. We provide a wide range of qualifications including academic, vocational, occupational and specific programmes for employers. For further information visit our qualifications websites at [www.edexcel.com](http://www.edexcel.com) or [www.btec.co.uk](http://www.btec.co.uk). Alternatively, you can get in touch with us using the details on our contact us page at [www.edexcel.com/contactus](http://www.edexcel.com/contactus).

**Pearson: helping people progress, everywhere**

Pearson aspires to be the world’s leading learning company. Our aim is to help everyone progress in their lives through education. We believe in every kind of learning, for all kinds of people, wherever they are in the world. We’ve been involved in education for over 150 years, and by working across 70 countries, in 100 languages, we have built an international reputation for our commitment to high standards and raising achievement through innovation in education. Find out more about how we can help you and your students at: [www.pearson.com/uk](http://www.pearson.com/uk)

Summer 2019

Publications Code 8MA0\_02\_1906\_MS

All the material in this publication is copyright
© Pearson Education Ltd 2019

**General Marking Guidance**

• All candidates must receive the same treatment. Examiners must mark the first candidate in exactly the same way as they mark the last.

• Mark schemes should be applied positively. Candidates must be rewarded for what they have shown they can do rather than penalised for omissions.

• Examiners should mark according to the mark scheme not according to their perception of where the grade boundaries may lie.

• There is no ceiling on achievement. All marks on the mark scheme should be used appropriately.

• All the marks on the mark scheme are designed to be awarded. Examiners should always award full marks if deserved, i.e. if the answer matches the mark scheme. Examiners should also be prepared to award zero marks if the candidate’s response is not worthy of credit according to the mark scheme.

• Where some judgement is required, mark schemes will provide the principles by which marks will be awarded and exemplification may be limited.

• When examiners are in doubt regarding the application of the mark scheme to a candidate’s response, the team leader must be consulted.

• Crossed out work should be marked UNLESS the candidate has replaced it with an alternative response.

# PEARSON EDEXCEL GCE MATHEMATICS

**General Instructions for Marking**

1. The total number of marks for the paper is 60.
2. These mark schemes use the following types of marks:
* **M** marks: Method marks are awarded for ‘knowing a method and attempting to apply it’, unless otherwise indicated.
* **A** marks: Accuracy marks can only be awarded if the relevant method (M) marks have been earned.
* **B** marks are unconditional accuracy marks (independent of M marks)
* Marks should not be subdivided.
1. Abbreviations

These are some of the traditional marking abbreviations that will appear in the mark

schemes.

* + **bod** – benefit of doubt
	+ **ft** – follow through
	+ the symbol will be used for correct ft
	+ **cao** – correct answer only
	+ **cso** - correct solution only. There must be no errors in this part of the question to obtain this mark
	+ **isw** – ignore subsequent working
	+ **awrt** – answers which round to
	+ **SC**: special case
	+ **o.e.** – or equivalent (and appropriate)
	+ **d** or **dep** – dependent
	+ **indep** – independent
	+ **dp** decimal places
	+ **sf** significant figures
	+ The answer is printed on the paper or ag- answer given
1. All M marks are follow through.

A marks are ‘correct answer only’ (cao.), unless shown, for example, as A1 ft to indicate that previous wrong working is to be followed through. After a misread however, the subsequent A marks affected are treated as A ft, but answers that don’t logically make sense e.g. if an answer given for a probability is >1 or <0, should never be awarded A marks.

be awarded A marks.

5. For misreading which does not alter the character of a question or materially simplify it, deduct two from any A or B marks gained, in that part of the question affected.

6. Where a candidate has made multiple responses and indicates which response they wish to submit, examiners should mark this response.

If there are several attempts at a question which have not been crossed out, examiners should mark the final answer which is the answer that is the most complete.

7. Ignore wrong working or incorrect statements following a correct answer.

8. Mark schemes will firstly show the solution judged to be the most common response expected from candidates. Where appropriate, alternatives answers are provided in the notes. If examiners are not sure if an answer is acceptable, they will check the mark scheme to see if an alternative answer is given for the method used. If no such alternative answer is provided but the response is deemed to be valid, examiners must escalate the response for a senior examiner to review.

**General Principles for Mechanics Marking**

*(But note that specific mark schemes may sometimes override these general principles)*

• Rules for M marks: correct no. of terms; dimensionally correct; all terms that need resolving (i.e. multiplied by cos or sin) are resolved.

• Omission or extra g in a resolution is an accuracy error not method error.

• Omission of mass from a resolution is a method error.

• Omission of a length from a moments equation is a method error.

• Omission of units or incorrect units is not (usually) counted as an accuracy error.

• DM indicates a dependent method mark i.e. one that can only be awarded if a previous specified method mark has been awarded.

• Any numerical answer which comes from use of g = 9.8 should be given to 2 or 3 SF.

• Use of g = 9.81 should be penalised once per (complete) question.

N.B. Over-accuracy or under-accuracy of correct answers should only be penalised *once* per complete question. However, premature approximation should be penalised every time it occurs.

• Marks must be entered in the same order as they appear on the mark scheme.

• In all cases, if the candidate clearly labels their working under a particular part of a question i.e. (a) or (b) or (c),……then that working can only score marks for that part of the question.

• Accept column vectors in all cases.

• Misreads – if a misread does not alter the character of a question or materially simplify it, deduct two from any A or B marks gained, bearing in mind that after a misread, the subsequent A marks affected are treated as A ft

• Mechanics Abbreviations

M(A) Taking moments about A.

N2L Newton’s Second Law (Equation of Motion)

NEL Newton’s Experimental Law (Newton’s Law of Impact)

HL Hooke’s Law

SHM Simple harmonic motion

PCLM Principle of conservation of linear momentum

RHS, LHS Right hand side, left hand side.

**8MA0 22: Mechanics AS 1906 Mark Scheme**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Question** | **Scheme** | **Marks** | **AOs** | **Notes** |
| **1 (a)** | *V* = 30 ()  | B1 | 3.4 | cao |
|  | **(1)** |  |  |
| **(b)** |  30  shape  figs 0 3 5 *T* |  B1 | 1.1b | Overallshape of the graph, starting at the origin.Dotted vertical line at end is OK but solid vertical line is B0 |
| B1**ft** | 1.1b | 3, 5 and *T* marked on the *t*-axis, and **ft** on their 30marked on the speed axis.3 must be where graph reaches a peak.Allow delineators: 3, 2 and *T* – 5 or a mixture |
|  |  | **(2)** |  |  |
| **(c)** | Using total area = 550 to set up an equation in **one unknown,**Or they may use *suvat* on one or more of the sections (but must still be considering all sections)M0 if they use one *suvat* equation for the whole motion | M1 | 2.1 | Need all sections to be included, with correct structure for each section. e.g. triangle + trapezium + rectangle oe = 550 to give an equation in **one unknown (may not be *T)*** |
|   **OR**:  **OR:**  |  A2 **ft** | 1.1b | **ft** on their answer to (a).-1 each error.**N.B.** If ‘6’ is incorrect, treat as one error, unless it is correct ft from their 30. |
| Solve for *T* | M1 | 1.1b | Attempt to solve for *T* provided they have tried to find the area using at least 3 sections.(M0 if they only solve for their unknown and never try to find *T*) |
| *T* = 83 (nearest whole number) | A1 | 1.1b | 83 is the only answer |
|  | **(5)** |  |  |
| **(d)** | New value of *T* would be bigger (ignore their reasons whether correct or not) | B1 | 3.5a | Clear statement about the value of *T*Allow ‘*it* would increase, get larger etc’B0 for ‘Takes longer’ or ‘the value of *T* would be longer’ |
|  |  | **(1)** |  |  |
| **(e)** | e.g. effect of wind; allow for dimensions of parachutist; use a more accurate value for *g*; parachutist does not fall vertically after chute opens; smooth changes in *v;* time for parachute to open; deceleration not constant (but B0 if they say *acceleration* not constant); smooth changes in *a;* B0 for: moves horizontally; mass/weight of parachutist; upthrust; air pressure;air resistance; terminal velocity | B1 | 3.5c | Any appropriate refinement of the model.B0 if incorrect (or irrelevant) extras |
|  |  | **(1)** |  |  |
| **(10 marks)** |  |

**N.B.** Omission or extra *g* in a resolution is an accuracy error not a method error

 In 2(a), use the mass which appears in the ‘*ma*’ term of an equation of motion, to identify which particle that equation of motion applies to.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Question** | **Scheme** | **Marks** | **AOs** | **Notes** |
| **2(a)** | Equation of motion for *Q* | M1 | 3.3 | Equation of motion for *Q* with correct no. of terms, condone sign errors. |
|   | A1 | 1.1b | A correct equation |
| Equation of motion for *P* | M1 | 3.3 | Equation of motion for *Q* with correct no. of terms, condone sign errors. |
|   | A1 | 1.1b | A correct equation |
|  \* | A1\* | 2.2a | Given acceleration obtained correctly. **You must see an equation in *a* only before reaching** ***a* = 4.2** |
|  | **(5)** |  | **N.B.** if they just use the whole system equation:, can only score max M1A1M0A0A0**N.B**. Use of *g* = 9.81 or 10 loses final A mark only.**N.B.**  Complete verification, using both equations, can score full marks. |
| **(b)** |  or e.g. they may find *v* first and then use *v* = 4.2  | M1 | 2.1 | Complete method (they may use more than one *suvat* equation) to find time for *Q* to hit the floor (M0 if 0.4 **not** used as distance moved and/or if 4.2 is **not** used as acceleration and this applies to finding *v* as well if they use *v* to find ) |
| (4357…..) Allow 0.43, 0.44, 0.436, or better, or any surd form e.g.   | A1 | 1.1b | See alternatives |
|   or 0.4 =  (*v* = 1.8330…) | M1 | 3.4 | Complete method to find speed of *Q* as it hits the floor(M0 if 0.4 **not** used as distance moved and/or if 4.2 is **not** used as acceleration and this applies to finding  as well if they use  to find *v*) |
|   | M1 | 1.1b | Uses distance/speed to find time for *P* to hit the pulley after *Q* has hit the floor.N.B. This is independent of previous M mark. |
| Complete strategy to solve the problem by finding the sum of the two times   |  **DM**1 | 3.1b | Complete method to solve the problem by finding and adding the two required times, dependent on previous three M marks |
| 1.0 (s) or 1.04 (s) | A1 | 1.1b |  |
|  | **(6)** |  |  |
| **(c)** | e.g. rope being light; rope being inextensible; pulley being smooth; pulley being small; balls being particles | B1 | 3.5b | Clear statement. Allow negatives of these i.e. the rope may not be light, the rope may not be inextensible etcMust be a limitation of the model stated in the questionPenalise incorrect or irrelevant extras |
|  |  | **(1)** |  | B0 for: Air resistance, table being smooth |
| **(12 marks)** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Question** | **Scheme** | **Marks** | **AOs** | **Notes** |
| **3(a)** | = 0 and solving | M1 | 3.1a | Equating *v* to 0 and solving the quadraticIf no evidence of solving, and at least one answer wrong, M0 |
|  | *t* = 6 (or -2) | A1 | 1.1b | 6 but allow -2 as well at this stage |
|  | Differentiate *v* wrt *t* | M1 | 1.1a | For differentiation (both powers decreasing by 1)  |
|  |   | A1 | 1.1b | Cao; only need RHS |
|  | When *t* = 6, *a* = - 8; Magnitude is 8 () | A1 | 1.1b | Substitute in *t* = 6 and get 8 (m s-2) as the answer .Must be **positive.** (A0 if two answers given) |
|  |  | **(5)** |  |  |
| **(b)** | Integrate *v* wrt *t* | M1 | 3.1a | For integration (at least two powers increasing by 1) |
|  |   | A1 | 1.1b | Correct expression (ignore *C*) only need RHSMust be used in part (b) |
|  | *t* = 3 => distance = 45 (m) | A1 | 1.1b | Correct distance. Ignore units |
|  |  | **(3)** |  |  |
| **(8 marks)** |  |

Pearson Education Limited. Registered company number 872828

with its registered office at 80 Strand, London, WC2R 0RL, United Kingdom